BUS ERROR INVESTIGATION RESULTS:

The following are the tasks done with observation results.

TASK 1 : DM with IP only.

**Observation:** Working fine.

**Issue :** continuous discovery command results in Segmentation Fault.

TASK 2 : DM with BLE only.

**Observation :** Raspberry Pi unable to detect IOTIVITY BLE SERVER.

TASK 3 : Both the above mentioned Tasks.

Observation : As Mentioned, only IP is working.

TASK 4 : DM with NON-IOTIVITY

**Observation :**  Working fine.

**More Details :** Out of 20 Times

2 Bus Errors

8 Segmentation Faults

10 Normal Working

**Issue :** continuous discovery command results in Segmentation Fault.

**Note :** A minimum of 1GB free space is considered while investigating Bus Error in Raspberry Pi.